**Type 1: Small conference room (TesiraFORTÉ AVB VT)**

* Up to (10) analog mics
* Stereo program audio
* USB soft codec VTC
* VoIP + POTS phone line options
* (6) Audio outs for spk zones + recording

**Type 2: Mid Sized conf room: VoIP, hard/soft VTC & mic logic (TesiraFORTÉ AVB VT + AVB CI)**

* (20) Analog table mics with switch, Red, Green per mic
* Stereo program audio
* Stereo hard codec VTC & USB soft codec VTC
* VoIP + POTS phone line options
* (6) Audio outs for spk zones + VTC

**Type 3: Small Dante mic conference room (TesiraFORTÉ DAN VT)**

* Up to (12) mic elements/lobes
* Stereo program audio
* Stereo hard codec VTC & USB soft codec VTC
* VoIP + POTS phone line options
* (6) Audio outs for spk zones + VTC

**Type 4: Medium Dante mic conference room (TesiraFORTÉ DAN VT + DAN CI)**

* Up to (24) mic elements/lobes
* Stereo program audio
* Stereo hard codec VTC & USB soft codec VTC
* VoIP + POTS phone line options
* (6) Audio outs for spk zones + VTC

**Type 5: 3-Way combine/divide Dante mic: VoIP & hard codec ((2) Tesira SERVER I/O AVB + DAN-1)**

* (2) Shure MXA910 ceiling mics (up to 8 lobes each) per room
* (4) Wireless mics (analog) per room
* Stereo program audio per room
* (1) Analog phone line per room
* (3) spk zones + VTC per room

**Type 6: (81) Auditorium: ((2) Tesira SERVER I/O AVB + TesiraFORTÉ AVB VT)**

* (74) Table mics, (5) Rack mics, (2) Wireless mics
* (1) Analog POTS Conferencing line
* Program Audio & Aux in
* (6) Ceiling speaker zones + Record & overflow feeds